**COMPUTER NETWORKS**


**NAME: M.ISTAFA MALIK**

**ROLL: P190033**

**SECTION: BSCS-5A**


**Solution:**


**Topology:**


****

**PC Configuration:**


**Assign Static IP’s to the PC’s**


****

****


****


**Server Configuration: Using static IP’s**


****


****

**Router Configuration:**

****

****


****

****


**Configure Dynamic NAT:**

4 STEPS:


1:

****


**2:**

****


**3:**


****

**4:**


****


# Testing Dynamic NAT Configuration Using Ping Command:






**THEN:**







**Done!**